|  |  |  |
| --- | --- | --- |
| **Category** | **Canvas elements** | **Construction & plates** |
| Zip top | Front, back; lip is printable on both sides | SW – 1 plate |
| Zip top with round hang hole | Front, back; lip is printable on both sides | SW – 1 plate |
| Zip top with sombrero hang hole | Front, back; lip is printable on both sides | SW – 1 plate |
| Slider top | Front, back | SW – 1 plate ? |
| Layflat | Front, back | BS - 2 plates - always or it depends? |
| Side gusset | Front, back | BS – 2 plates |
| Auto bags (aka pre-opened bags on rolls) | Front, back | BS – 2 plates |
| Wicketed layflat | Front, including lip - show 2 wicket holes (distance between holes = wicket width?); back | SW – 1 plate |
| Wicketed bottom gusset | Front, including lip - show 2 wicket holes (distance between holes = wicket width?); back; bottom gusset | SW – 1 plate |
| Lip & tape, permanent | Front (including lip) and back; we will also depict the non-printable area (area from the back opening down, that the lip folds over onto). Also: show tape in preview & tech drawings for back side. | SW – 1 plate |
| Lip & tape, resealable Any visual difference between permanent and resealable tape? If not, canvases for permanent and resealable can be the same? | Front (including lip) and back; we will also depict the non-printable area (area from the back opening down, that the lip folds over onto). Also: show tape in preview & tech drawings for back side. | SW – 1 plate |
| Poly mailers (aka co-extruded) – non-perforated | Front (including lip) and back; always full bleed, so no "safe-line." Also: show tape in preview & tech drawings for back side. | SW – 1 plate |
| Poly mailers (aka co-extruded) – perforated | Front (including lip, show perforation line) and back; always full bleed, so no "safe-line." Also: show tape in preview & tech drawings for back side. | SW – 1 plate |
| Poly mailers (aka co-extruded) - returnable | Front (including lip, show two perforation lines) and back; always full bleed, so no "safe-line." Also: show both tape strips in preview & tech drawings for back side. | SW – 1 plate |