|  |  |  |
| --- | --- | --- |
| **Category** | **Canvas elements** | **Construction & plates**  |
| Wicketed layflat  | Front.Back, including lip - show 2 wicket holes (distance between holes = wicket width). Note: no printing on lip of wicketed bags – to be indicated by position of safety line.We also need to illustrate chosen bag release option (tear start or perforated lip) in designer and preview (as we do now in tech drawings). | SW – 1 plate |
| Wicketed bottom gusset | Front, with safety lines for sides, top and bottom. Back, including lip - show 2 wicket holes (distance between holes = wicket width). Note: no printing on lip of wicketed bags; indicate with height of safety line. Bottom gusset; safety lines at sides only.As stated above, we also need to illustrate chosen bag release option. | SW – 1 plate |
| Lip & tape, permanent  | Long side (including lip). Safety lines on sides, top and bottom. Line indicating lip.Short side (see below) showing flip side of the lip (interior of bag with tape – tape is white ). Depict the non-printable area (area from the top of the opening down, that the lip folds over onto) with safety line. TBD whether other indicators are necessary like watermark text “Non-printable area.” | SW – 1 plate |
| Lip & tape, resealable  | Same as above except the resealable tape is clear. | SW – 1 plate |
| Poly mailers (aka co-extruded) – non-perforated | **Film exterior is white.**Long side (including lip)Short side (see below) showing flip side of the lip (interior of bag with clear tape).Both sides: always full bleed, so no "safety line."\*\* \*\*Jay to confirm: Should we have a nonprintable area for where the lip folds over onto the short side? In any case, no safety lines on sides or bottom of short side; no safety lines on top, sides or bottom of long side.  | SW – 1 plate |
| Poly mailers (aka co-extruded) – perforated | Same as above but depicting perforation in addition to tape strip.Short side: | SW – 1 plate |
| Poly mailers (aka co-extruded) - returnable | Same as above but depicting two clear tape strips and two perforations. | SW – 1 plate |
| Zip top | Front (including zipper and lip), back (including zipper and lip). Safety lines on sides, top, bottom of lip and sides, top, bottom of front/back. | SW – 1 plate  |
| Zip top with round hang hole | Same as zip top above with centered, round X” hang hole shown on front and back of lip.  | SW – 1 plate |
| Zip top with sombrero hang hole | Same as zip top above with centered sombrero hole shown on front and back of lip. | SW – 1 plate |
| Slider top  | Front (including slider), back (including slider); safety lines sides, top and bottom. | SW – 1 plate |
| Layflat  | Front, back. Safety lines on sides, top and bottom.  | SW – 1 plate |
| ~~Side gusset~~ - PHASE 2 | ~~Front, back, gusset lines~~ | ~~BS – 2 plates~~ |
| ~~Auto bags (aka pre-opened bags on rolls)~~ - PHASE 2 | ~~Front, back~~ | ~~BS – 2 plates~~ |