**Marketplace Template**

Description: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Lip & Tape Pricing Model\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. New Catalog Code or Existing? If new, where should it be placed in Level 2 menu?
   * 1. New catalog code. Please see “Nested Category Dropdowns” for where it should be placed in the menus.
2. Widget Level 2 Enabled? If Yes:
   * 1. Width ranges:4”-30”
     2. Depth enabled? **Phase 2:** Depth Ranges: 1”-8” \*The depth is not a side gusset. It is a bottom gusset. It must be less than length.
     3. Length ranges: 5”-32”
     4. We will need a field for the lip. **Phase 1 to be handled in “Nested Category Dropdowns” Phase 2:** customers should be able to change the lip size between the range of 0.5”-6.0”
     5. Gauge ranges: 1-4 mill
     6. Full gauge allowed? Default? Full gauge should be allowed and should increase the cost, but nominal should be default.
3. Widget Level 3 Enabled? (Be specific)
   1. Material Menu Enabled? Which options are allowed for Materials and Additives? What is the default?
      1. Yes, **Phase 1 to be handled in “Nested Category Dropdowns”. Phase 2:** the customer needs to be able to select either permanent tape or resealable tape. They should also have the option to select postal approved in conjunction with permanent tape.
   2. Color Menu Enabled? All colors/opacity allowed? What is the default?
      1. None. Clear film only to start.
   3. Printing Menu Enabled?
      1. **Phase 2:** Yes. Customers should be able to select random repeat printing. This includes custom plates, and also the two stock suffocation warnings (24 font + 14 font stock suffocation warnings)
   4. Venting Menu Enabled? Which options? Nbr of Holes Min/Max? Any defaults? No defaults.
      1. 1-4 vent holes enabled. 1/4” & 1/8”
   5. Packaging Enabled? What is the default?
      1. Cases only. Case weight between 13-32 pounds preferably.
4. Minimum Quantity calculation:
   * 1. =((13750/91.67)/WIDTH)\*(order conversion constant dependent on gauge)
5. Customer Pricing/Vendor Costing Model – provide calculation or Excel Spreadsheet::
   * 1. Excel sheet available
6. Standard Quantity Break calculation (if any):
   * 1. 2x minimum
     2. 4x minimum
     3. 6x minimum
7. Case or Roll Weight calculation (including packaging) – if on a roll, we need the core weight as well as the box weight. If in a case, we need the box weight:
   * 1. =(((width\*(length+(0.5\*lip)+(0.5\*gusset))\*gauge)/15)\*(number of bags in a case/1000))+standard box weight
8. Freight Calculation (include ‘from’ warehouse and carrier if using standard freight tables). Do we allow shipments to Canada?
   * 1. Please calculate shipping from Reno Nevada only using YRC as the carrier.
9. Is Freight always included in the price (disable freight option)?
   * 1. To keep it simple and safe, freight should always be included in the price
10. Lead Time Days:
    * 1. 32 days.
11. Should Import result be shown?
    * 1. No.
12. Overrun Percentage:
    * 1. Less than 30M +/- 25%
      2. 30M-60M +/- 20%
      3. 60-150M +/- 15%
      4. +150M +/- 10%
13. Additional text in quote/order item description?

Derived from “Nested Category Dropdowns”

* 1. Tape Type: Permanent or Resealable
  2. Material: Polyethylene, Polypropylene, or Postal Approved
  3. Lip Size